# Sludge-Dewatering Device (SCHLAMMCON) page 1 / 1

STANDARD VERSION

|  |  |
| --- | --- |
| design | solid welding |
| material | steel - galvanized |
| side parts in trelliswork |  |
| inside lined with filter-fleece, top open |  |

|  |  |
| --- | --- |
| The bottom of the device is to open up, unlocking for opening the bottom  plate manual by an outside lock.  In the range of the top shoes are integrated for picking up the device by a forklift truck. | |
|  |  |
| dimension | 1100 x 1100 x 1150 mm |
| bottom hole | each 500 x 1.000 mm |

|  |  |
| --- | --- |
| **Effluent-Collector** |  |
| with pedestal for the SCHLAMMCON |  |
| as well as discharge pipe for filtrate outflow |  |
|  | |
| material | polypropylene |

|  |  |
| --- | --- |
| Manufacturer | Dango & Dienenthal Filtertechnik GmbH |
|  | +49 271 401 41 23 |